DiagMgr UnitTest Notes for Developer

(Note: Below is for short term plans. Long term plan is to make TEST\_CFG folder more generic for projects)

To complete DiagMgr Unittest, DiagMgr files in GenData folder(DiagMgr\_Cfg.c, DiagMgr\_Proxy.c) should also be unit tested. These files are different across projects. Below steps should be followed to send files to ODC

1. Place files from GenData ((DiagMgr\_Cfg.c, DiagMgr\_Proxy.c) in TEST\_CFG folder of integration project .(For eg: BMW\_UKL\_MCV\_EPS\_TMS570\Tessy\Reports\DiagMgr).
2. While submitting DiagMgr component to ODC for unittest, place TEST\_CFG folder from step 1 in utp/contract folder of DiagMgr component(DiagMgr\utp\contract)
3. And reports of DiagMgr component should be placed in integration project.(For eg: BMW\_UKL\_MCV\_EPS\_TMS570\Tessy\Reports\DiagMgr)